# Visual System

Style name: Energy Grid Control

## Core DNA

- Deep navy, almost black, background with a faint electric-blue circuit lattice and a low city silhouette along the bottom.
- Glowing blue line-art transmission towers at the far left and right joined by catenary power lines.
- Wind turbine, tilted solar array and a small solar-yellow sun glyph tucked into the top corners only.
- Massive white Japanese gothic headline with a hard navy keyline, soft electric-blue outer glow and solar-yellow final characters.
- One clipped-corner subline banner outlined in a thin cyan hairline, white type with solar-yellow emphasis, flanked by tiny node-and-link diagrams.
- Translucent dark console plates with clipped notch corners and thin glowing borders in electric blue, signal green and solar yellow.
- Exactly three hexagon-notched neon label plates docked below the panels, white Japanese lettering with a solid icon badge at the left.
- Solar-yellow chevron arrows with a soft glow carrying current between panels.
- Instrument scenes lit from within: load bars, donut gauges, rising line charts, breaker and meter glyphs, all flat vector with controlled glow.
- One full-width bottom band bordered by a cyan hairline with solar-yellow emphasis words, a glowing pylon at the left and substation and city-block icons with green level bars at the right.

## Intended Use

電力、設備、脱炭素、インフラ制御をテーマにしたスライドに使う。電力網、需要予測カード、設備パネルで安定運用の緊張感を出し、暗い画面でも数値と状態が一目で読める構成にする。

## Page Architecture

- One oversized headline.
- One subline banner.
- One dominant diagram occupying most of the body.
- Exactly three labels.
- One takeaway band.
- Three to six supporting icons that explain the diagram.

## Composition Grammar

- Cover: title wall with the three glowing console plates previewing the three labels, pylons at both edges, renewables in the top corners and the cyan-hairline band anchoring the bottom.
- Problem: interrupted feeder halted at three pulsing fault points with overload gauges.
- Before-after: strained single feeder resolving into an automated dispatch circuit and a human supervisory circuit.
- Three-step: three console plates as generation, transmission and consumption stages joined by glowing chevrons.
- Loop: closed generation-storage-dispatch-metering ring with a state-of-charge gauge at its center.
- Checklist: switchgear commissioning panel with three oversized check rows and certification tags.
- Roadmap: transmission corridor strung between three pylon milestones toward an energized district.
- Matrix: 2x2 dispatch priority board with one energized solar-yellow quadrant and a lightning bolt.
- Case: 24-hour demand curve band with morning ramp, solar peak and evening shave markers.
- Recap: central dispatch-desk plate with three stacked switching orders and a radial power-flow diagram.
