# Visual System

Style name: Logistics Control Tower

## Core DNA

- Near-black dark slate background with a faint dotted world-map texture behind everything.
- Dim photographic night port and truck yard bleeding in from the left and right edges, never in the center.
- Dashed safety-orange and white route arcs across the top with small flat plane, truck and ship glyphs and teal waypoint dots.
- Massive extruded Japanese gothic headline, warm white with the final characters in safety orange, thick dark keyline and a slight bevel.
- One teal-outlined subline bar with orange emphasis words, a warehouse icon at its left end and a chart icon at its right.
- Dark charcoal panels with notched corner cuts and thin 1px borders in safety orange, teal and signal yellow.
- Exactly three solid colored label bands clamped across panel bottoms, white Japanese lettering plus a small outlined icon.
- Solid chevron arrows in safety orange and teal driving movement between panels.
- Left and right margin rails of small monitoring widgets: KPI tiles with up/down arrows, donut charts with legends, orange alert triangles, horizontal status bars, mini line charts.
- One full-width dark takeaway band with a teal hairline border, orange emphasis words, a signaling control tower on the left and a container ship on the right.

## Intended Use

物流、倉庫、配送管理、在庫オペレーション向けのスライドに使う。ルート線、倉庫カード、例外アラートで管制塔から現場全体を見ている感覚を出し、数字と状態が同時に読める構成にする。

## Page Architecture

- One oversized headline.
- One subline banner.
- One dominant diagram occupying most of the body.
- Exactly three labels.
- One takeaway band.
- Three to six supporting icons that explain the diagram.

## Composition Grammar

- Cover: title board with the three numbered dispatch panels previewing the three labels, full margin rails of monitoring widgets, route arcs overhead and the control tower anchoring the bottom band.
- Problem: clogged trunk route stopped at three orange exception markers with climbing delay counters.
- Before-after: tangled manual dispatch board resolving into an automated routing lane and a human review lane.
- Three-step: three notched dispatch panels as consecutive conveyor stations joined by chevrons.
- Loop: closed outbound and empty-return circulation loop through three relay hubs with a cycle-time gauge.
- Checklist: dock-door pre-departure manifest panel with three oversized check rows and status stamps.
- Roadmap: dashed shipping lane from origin port to destination port past three transit hub markers.
- Matrix: 2x2 routing priority board with one lit signal-yellow quadrant and a priority-lane star.
- Case: 24-hour operations timeline band with three shift markers stitched by a dotted route line.
- Recap: central control-tower console card with three stacked dispatch tickets and a radar sweep.
